For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .
2. Disconnect the harness connector.
3. Remove the 2 screws and the actuator.

### Installation Procedure

1. Position the actuator and install the 2 screws.
2. Connect the harness connector.
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .