For 1990-2009 cars

## Park/Turn Signal/Side Marker Lamp Replacement Front

### Removal Procedure

1. Remove the screws (1) from the sidemarker lamp (2).
2. Remove the sidemarker lamp (2) from the front fascia panel (5).
3. Remove the socket (4) from the sidemarker lamp (2).
4. Remove the bulb (3) from the socket (4).

### Installation Procedure

1. Install the bulb (3) to the socket (4).
2. Install the socket (4) to the sidemarker lamp (2).
3. Install the sidemarker lamp (2) to the front fascia panel (5).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the screws (1) to the sidemarker lamp (2).

Tighten
Tighten the screws to 2 N·m (18 lb ).

## Park/Turn Signal/Side Marker Lamp Replacement Rear

### Removal Procedure

1. Remove the taillamp. Refer to Tail Lamp Replacement .
2. Disconnect the electrical connector (7).
3. Remove the bulb (5) from the socket (5).

### Installation Procedure

1. Install the bulb (5) to the socket (5).
2. Connect the electrical connector (7).
3. Install the taillamp. Refer to Tail Lamp Replacement .