For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6C FUEL SYSTEM INFORMATION

#### SUBJECT: SERVICE MANUAL UPDATE FUEL PRESSURE RELIEF REVISED PROCEDURE

#### MODELS/YEARS: 1989-91 CUTLASS CALAIS, CUTLASS CIERA AND CUTLASS CRUISER W/2.3L, 2.5L & 3.3L (VIN A, D, U, R, N) ENGINES

This information replaces Fuel System Pressure Relief Procedures found in the following service manuals:

1989-91 Cutlass Ciera/Cruiser with 2.5L (VIN R)

1989-91 Cutlass Calais with 2.5L (VIN U)

1991 Cutlass Calais with 2.3L (VIN A and D) and 3.3L (VIN N)

#### CAUTION:

To reduce the risk of fire and personal injury, relieve the fuel system pressure before servicing fuel system components. After relieving system pressure, a small amount of fuel may be released when servicing fuel lines or connections. To reduce the chance of personal injury cover fuel line fittings with a shop towel before disconnecting, to catch any fuel that may leak out. Place the towel in an approved container when disconnect is completed.

Fuel pressure relief procedure: 1989-91 2.3L (VIN A and D) and 2.5L (VIN R and U)

1. Loosen fuel filler cap to relieve tank pressure (Do not re-tighten at this time). 2. Raise vehicle. 3. Disconnect fuel pump electrical connector. 4. Lower vehicle. 5. Start engine and run until fuel supply remaining in fuel pipes is consumed. Engage starter for 3.0 seconds to assure relief of any remaining pressure. 6. Raise vehicle. 7. Connect fuel pump electrical connector. 8. Lower vehicle. 9. Disconnect negative battery terminal to avoid possible fuel discharge if an accidental attempt is made to start the engine.

3.3L (VIN N) Tool required: J 34730-1, Fuel Pressure Gage.

1. Disconnect negative battery terminal to avoid possible fuel discharge if an accidental attempt is made to start the engine.

2. Loosen fuel filler cap to relieve tank pressure (Do not re-tighten at this time).

3. Connect J 34730-1 to fuel pressure connection. Wrap a shop towel around fitting while connecting gage to avoid spillage.

4. Install bleed hose into an approved container and open valve to bleed system pressure. Fuel connections are now safe for servicing.

5. Drain any fuel remaining in gage into an approved container.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.