For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Turn ignition OFF.
2. Disconnect the windshield wiper motor connector.
3. Turn the ignition ON.
4. Set the wiper/washer switch to LO.
5. Connect a test light from wiper motor connector terminal E to ground.

Is the test light on?

--

Go to Step 6

Go to Step 3

3 | Connect a test light (backprobe) from terminal D at the wiper/washer switch connector to ground. Is the test light on? | -- | Go to Step 4 | Go to Step 5
4 | Repair the open in CKT 112 between the switch and the motor. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
5 | Replace the wiper/washer switch. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
6 | Measure the voltage from terminal D to ground at the windshield wiper motor connector using a J 39200. Is the voltage within the specified value? | 10.5-15 V | Go to Step 7 | Go to Step 8
7 | Replace the windshield wiper motor. Refer to Windshield Wiper Motor Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
8 | Measure the voltage from terminal E to ground at the wiper/washer switch connector using a J 39200. Is the voltage within the specified value? | 10.5-15 V | Go to Step 9 | Go to Step 5
9 | Repair the open in CKT 113 between the switch and the motor. Is the repair complete? | -- | Go to Wiper/Washer System Check | --