For 1990-2009 cars

# GM-GOODWRENCH 350 THM REMANUFACTURED TRANSMISSION

GM Parts & Accessories Bulletin 82-130 and 82-188 announced the availability of GM-Goodwrench 350 THM Remanufactured Transmissions.

Tht GM-Goodwrench 350 THM Remanufactured Transmission (26 separate part numbers) will replace approximately 475 service applications currently released for 1969 through 1981 model vehicles.

This transmission is attractively priced at $350.00 per unit (dealer net) plus $50.00 core charge. When specific quantities are ordered to earn a 10% to 15% discount, and the 8% return reserve and 3% advertising allowance is considered, the unit price can be as low as $259.00.

Each transmission is remanufactured using genuine GM quality replacement parys. Included is a 100% Rebuilt GM Torque Converter. Each transmission is backed with a 4,000 mile/90 day GM Warranty.

Part numbers for Oldsmobile applications are listed on the reverse side of this bulletin. Additional details are listed in the GMP&A bulletins listed above. Be sure your service management team is aware of this opportunity to assist your customers.

#### OLDSMOBILE

YEAR APPLICATION PART NUMBER ---- ----------- ----------- 1977 A (260F) (M38) 1978-80 A (260F) (M33) 1977 X (231C) (M38) 1978-79 B (260F) (M33) .......................... 14055075

1979 A, H (231A,2) (M33); X (231A) (M33) ..... 14055076

1979 A, (196) (M33); B(231A) (M33) 1980 A (231A) (M33) .......................... 14055077

1980 A, B (231A) (M38) 1980 H (M38) ................................. 14055078

1970-74 A, B, X, (L6) (M38) (B.O.P Eng) 1975-76 A (260) (M38) 1975 H (M38) 1976 H (231C) (M38) 1975-76 X (260) (M38) 1977 A, B, X (231C) (M38) 1977 H (231, A, C) (M38) 1978 A, B, H, X (231A) (M33) ................. 14055079

1978 B (350N) (M33) 1979 A, B, C (350N) (M33) 1980 A (301W,350R) (M33) ....... ............. 14055082

1969 A (V8) (M38) (B.O.P. Eng) 1970 A (V8) (M38) w/4BBL (B.O.P Eng) 1971-73 A, B (V8) (M38) (B.O.P. Eng) 1974 X (V8) (M38) (B.O.P. Eng)................ 14055085

1976 A (350R) (M38) w/2.41 ratio 1977 A (403) (M38) 1977 A (350R) (M38) w/alt. Calif. 1977 B, C (350R, 403) (M38) 1977 X (350R) (M38) 1979 B (350R) (M33) w/alt. 1979 B (403) (M33) w/3.23 ratio 1980 B (350R, X) (M33) ....................... 14005086

1980 A (267,305H) (M38) ...................... 14055087

1970 A (V8) (M38) w/2BBL (B.O.P. Eng) 1975 A (350R) (M38) 1975-76 X (350 H, X) (M38) 1976 A (350R) (M38) exc 2.41 ratio 1977 A (350R) (M38) exc alt. Calif 1979 B (350R) (M33) w/Fed 1979 B (403) (M33) w/2.41, 3.08 ratio ........ 14055088

1970 A (V8) (M38) w/2BBL 1976 B (350R) (M38) .......................... 14055089

1970-74 A, B, X (L6) (M38) (Chev. Eng) 1976-76 A, X (250) (M38) ........................ 14067504

1969 A (V8) (M38) (Chev. Eng) 1970 A (V8) (M38) w/4 BBL (Chev. Eng) 1971-73 A, B (V8) (M38) (Chev. Eng) 1974 X (V8) (M36) (Chev. Eng) ................ 14067505

1980 A(267,305H) (M33);B(305H) (M33) ......... 14067506

1970 A (V8) (M38) w/2BBL (Chev. Eng) 1978-79 A (305, 350L) (M33) 1978-79 X (305U, 350L) (M33) ................... 14067507

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.