For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Remove the tube bracket to the rear cam carrier lift bracket bolt.
3. Remove the tube from the block.

#### Installation Procedure

1. Install the tube to the block.
2. Install the tube bracket to the rear cam carrier lift bracket bolt.

Tighten
Tighten the bolt to 8 N·m (72 lb in).

3. Install the negative battery cable.