For 1990-2009 cars

#### Battery

(1) | Positive Battery Cable
(2) | Negative Battery Cable
(3) | Battery Ground
(4) | Engine Ground
(5) | Underhood Junction Block

#### Underhood Junction Block

(1) | Electrical Center Cap
(2) | Positive Battery Cable to Underhood Junction Block
(3) | Positive Battery Cable
(4) | Battery

#### LH Hand Rear of Engine Compartment

(1) | Brake Pressure Switch
(2) | Master Cylinder

#### Front of Engine Compartment

(1) | Switch, A/C Pressure
(2) | Connector, Fan Motor
(3) | To Main Engine Wiring Harness

#### Left Hand Rear of Engine Compartment

(1) | Brake Pressure Switch
(2) | To Underhood Junction Block
(3) | Grommet

#### Starter and Crankshaft Sensors

(1) | Positive Battery Cable
(2) | Fusible Link
(3) | Starter
(4) | Crankshaft Position (CKP) Sensor

#### Right Hand Side of Engine

(1) | Generator
(2) | Connector, Generator
(3) | Coolant Temperature Sensor
(4) | Camshaft Position

#### Right Hand Front of Engine

(1) | Generator
(2) | Generator Lead
(3) | Ground Splice Pack
(4) | Ground Splice Pack
(5) | Engine Wiring Harness
(6) | Canister Purge Solenoid
(7) | Connector, A/C Compressor
(8) | A/C Compressor
(9) | Connector, Generator

#### Front of Engine

(1) | Throttle Position Sensor (TPS)
(2) | Mass Air Flow Sensor (MAF)
(3) | Vacuum Tube
(4) | Idle Air Control (IAC) Valve

#### Top Front of Engine

(1) | Exhaust Gas Recirculation (EGR) Valve
(2) | Throttle Position Sensor (TPS)
(3) | Camshaft Position Sensor
(4) | Connector, Camshaft Position Sensor
(5) | Connector, Fuel Injector

#### Oxygen Sensor Lead

(1) | Connector, Oxygen Sensor
(2) | Coolant Vent Pipe
(3) | Exhaust Manifold

#### Left Hand Front of Engine

(1) | Engine Wiring Harness
(2) | Neutral Start Back-up Switch (NSBU)
(2) | Neutral Start Back-up Switch (NSBU)
(3) | Manifold Air Temperature (MAT) Sensor
(4) | To Cooling Fan Motors
(5) | Automatic Transaxle
(6) | To Starter Motor

#### Right Hand Rear of Engine

(1) | Transaxle Bracket
(2) | Vehicle Speed Sensor (VSS)
(3) | To Antilock Brake System
(4) | Heater Pipe

#### Lower Front of Engine

(1) | Radiator Hoses
(2) | Engine Wiring Harness

#### Rear of Engine

(1) | Engine Wiring Harness
(2) | Connector, Rear Oxygen Sensor

#### Left Hand Rear of Engine Compartment

(1) | Brake Pressure Switch
(2) | Engine Wiring Harness

#### Starter

(1) | To A/C Compressor
(2) | Positive Battery Cable
(3) | Starter Solenoid
(4) | Starter Solenoid Ground
(5) | Starter Assembly
(6) | Battery Positive

#### Left Hand Side of Engine

(1) | Battery Ground
(2) | Neutral Start Back-up Switch (NSBU)
(2) | Neutral Start Back-up Switch (NSBU)
(3) | Antilock Brake System (ABS)
(4) | Cooling Fan Lead
(5) | Automatic Transaxle

#### Front of Engine

(1) | Oil Pressure Sensor
(2) | Positive Battery Cable
(3) | Engine Wiring Harness
(4) | Engine Mount Bracket
(5) | Negative Battery Cable
(6) | Ground Splice Pack
(7) | Starter Motor Assembly
(8) | Oil Pan
(9) | Knock Sensor
(10) | A/C Compressor Clutch
(11) | A/C Compressor
(12) | Crankshaft Position Sensor
(13) | Water Pump

#### Top Rear of Engine

(1) | Camshaft Position Sensor
(2) | Coolant Temperature Sensor
(3) | Inline to Fuel Injectors
(4) | Electronic Ignition (EI) Module
(5) | Oxygen Sensor
(6) | Canister Purge Solenoid
(7) | Connector, Electronic Ignition (EI) Module

#### Right Hand Rear of Engine

(1) | Low Oil Level Sensor
(2) | To Antilock Brake System (ABS)
(3) | Vehicle Speed Sensor (VSS)