For 1990-2009 cars

# SMU - SECTION 6A5 REVISED PUSH ROD ID.

REVISION: 11/11/94

#### THIS BULLETIN WAS REVISED TO CHANGE THE MODELS SECTION.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A5 - REVISED PUSHROD IDENTIFICATION

#### MODELS: 1994-95 BUICK CENTURY, REGAL AND SKYLARK 1994-95 CHEVROLET BERETTA AND CORSICA 1995 CHEVROLET LUMINA AND MONTE CARLO 1993-95 OLDSMOBILE CUTLASS SUPREME 1994-95 OLDSMOBILE ACHIEVA AND CUTLASS CIERA 1994-95 PONTIAC GRAND AM AND GRAND PRIX WITH 3100 ENGINE (VIN M - RPO L82)

THE PUSHROD IDENTIFICATION FOR 3100 ENGINES (VIN M - RPO L82) HAS BEEN REVISED. USE THE FOLLOWING INFORMATION TO PROPERLY IDENTIFY THE PUSHRODS.

1993-95 3100 (L82) PUSHROD IDENTIFICATION - INTAKE VALVE PUSHRODS ARE PAINTED WITH TWO YELLOW STRIPES AND MEASURE 144.18 MM (5.68 INCHES) LONG.

- EXHAUST VALVE PUSHRODS ARE PAINTED WITH TWO GREEN STRIPES AND MEASURE 152.51 MM (6.0 INCHES) LONG.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.