For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Align the notch in the outside rearview mirror remote control bezel (1) with the tab in the hole at the front of the armrest.
3. Push on the base of the outside rearview mirror remote control bezel in order to remove the bezel from the door trim panel.

### Installation Procedure

1. Align the notch in the outside rearview mirror remote control bezel (1) with the tab in the hole at the front of the armrest.
2. Push on the outside rearview mirror remote control bezel (1) in order to secure the bezel.
3. Install the door trim panel. Refer to Door Trim Panel Replacement .