For 1990-2009 cars

Problem | Action
--- | ---
A worn cancel cam | Replace the components as necessary. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
The detent spring exhibits one of the following conditions:

• | Broken

• | Missing

• | Out of position

Adjust or replace the spring as necessary.

Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .

The return spring exhibits one of the following conditions:

• | Broken

• | Missing

• | Out of position

Adjust or replace the spring as necessary.

Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .

The cancel spring exhibits one of the following conditions:

• | Broken

• | Missing

• | Out of position

Adjust or replace the spring as necessary.

Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .

Loose switch mounting screws | Tighten the screws to specification. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
A broken switch | Repair the components as necessary. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
Broken anchor bosses | Repair the components as necessary. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .