For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the front wheelhouse panel liner retainers (4).
4. Remove the front wheelhouse panel liner screws (2).
5. Remove the front wheelhouse panel liner (3).

### Installation Procedure

1. Install the front wheelhouse panel liner (3).
2. Install the front wheelhouse panel liner screws (2).
3. Install the front wheelhouse panel liner retainers (4).
4. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
5. Lower the vehicle.