For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Backprobe the hazard switch connector with a test lamp betwen terminal G and ground.
2. Turn the ignition switch to the ON position.
3. Turn the right turn signal ON.

Does the test lamp flash?

--

Go to Step 3

Go to Step 4

3 | Replace the hazard switch. Refer to Hazard Flasher Switch Replacement in Instrument Panel, Gauges and Console. Is the repair complete? | -- | Go to Exterior Lights System Check | --
4 | Repair the open in CKT 15 between the hazard switch and the right IP wiring harness junction block. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Disconnect the hazard switch connector.
2. Connect a test lamp between terminal B of the hazard switch connector and ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Connect a test lamp between terminal B and terminal A of the hazard switch connector. Does the test lamp light? | -- | Go to Step 5 | Go to Step 6
4 | Backprobe the left IP junction block connector C1 with a test lamp between terminal C12 and ground. Does the test lamp light? | -- | Go to Step 7 | Go to Step 8
5 | Replace the hazard switch. Refer to Hazard Flasher Switch Replacement in Instrument Panel, Gauges and Console. Is the repair complete? | -- | Go to Exterior Lights System Check | --
6 | Repair the open in CKT 150 between the hazard switch and ground splice pack G201. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --
7 | Repair the open in CKT 1140 between the hazard switch and the left IP junction block. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --
8 | Replace the left IP junction block. Refer to Relay/Fuse Center Replacement in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --