For 1990-2009 cars

DTC | Description | Domestic RPO L82 | Export Unleaded RPO L82 | Export Leaded
--- | --- | --- | --- | ---
P0101 | Mass Air Flow (MAF) System Performance | A | A | --
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | A | A | A
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | A | A | A
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | B | B | B
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | B | B | B
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | B | B | B
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | B | B | B
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | B | B | B
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | B | B | B
P0121 | Throttle Position (TP) System Performance | A | A | A
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | A | A | A
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | A | A | A
P0125 | Engine Coolant Temperature (ECT) Excessive Time to Closed Loop Fuel Control | B | D | --
P0131 | HO2S Circuit Low Voltage Sensor 1 | B | B | --
P0132 | HO2S Circuit High Votlage Sensor 1 | B | B | --
P0133 | HO2S Slow Response Sensor 1 | B | C | --
P0134 | HO2S Circuit Insufficient Activity Sensor 1 | B | B | --
P0135 | HO2S Heater Circuit Sensor 1 | B | D | --
P0137 | HO2S Circuit Low Voltage Sensor 2 | B | B | --
P0138 | HO2S Circuit High Voltage Sensor 2 | B | B | --
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | B | B | --
P0141 | HO2S Heater Circuit Sensor 2 | B | D | --
P0171 | Fuel Trim System Lean | B | D | --
P0172 | Fuel Trim System Rich | B | D | --
P0201 | Injector 1 Control Circuit | B | B | B
P0202 | Injector 2 Control Circuit | B | B | B
P0203 | Injector 3 Control Circuit | B | B | B
P0204 | Injector 4 Control Circuit | B | B | B
P0205 | Injector 5 Control Circuit | B | B | B
P0206 | Injector 6 Control Circuit | B | B | B
P0230 | Fuel Pump Control Circuit | D | D | D
P0300 | Engine Misfire Detected | B | D | --
P0325 | Knock Sensor Circuit | D | D | D
P0327 | Knock Sensor Circuit Bank 1 | D | D | D
P0336 | 18X Reference Signal | B | B | B
P0341 | CMP Sensor Circuit Performance | B | B | B
P0401 | EGR System Flow Insufficient | A | D | --
P0403 | EGR Solenoid Circuit | B | D | --
P0404 | EGR System Performance | B | D | --
P0405 | EGR Pintle Position Circuit Low Voltage | B | D | --
P0420 | TWC System Low Efficiency | A | D | --
P0440 | EVAP System | A | A | --
P0442 | EVAP Control System Small Leak Detected | A | A | --
P0446 | EVAP Canister Vent Blocked | A | A | --
P0452 | Fuel Tank Pressure Sensor Low Voltage | B | B | --
P0453 | Fuel Tank Pressure Sensor High Voltage | B | B | --
P0502 | VSS Circuit Low Input | B | B | D
P0503 | VSS Circuit--Intermittent Input | B | B | D
P0506 | Idle Control System Low RPM | B | B | B
P0507 | Idle Control System High RPM | B | B | B
P0530 | A/C Refrigerant Pressure Sensor Circuit | D | D | D
P0560 | System Voltage | D | D | D
P0601 | PCM Memory | B | B | B
P0602 | PCM Not Programmed | B | B | B
P0654 | Tachometer Control Circuit | D | D | D
P0705 | Trans Range Switch Circuit | D | D | D
P0706 | Trans Range Switch Performance | D | D | D
P0711 | Trans Fluid Temperature (TFT) Sensor Circuit Performance (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0712 | Trans Fluid Temperature (TFT) Sensor Circuit Low Voltage (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0713 | Trans Fluid Temperature (TFT) Sensor Circuit High Voltage (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0716 | Automatic Transmission Input (Shaft) Speed Sensor Circuit Performance (Refer to Automatic Transaxle Diagnosis) | B | B | D
P0717 | Automatic Transmission Input (Shaft) Speed Sensor No Input (Refer to Automatic Transaxle Diagnosis) | B | B | D
P0719 | Brake Switch Circuit Low (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0724 | Brake Switch Circuit High (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0730 | Incorrect Gear Ratio (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0741 | Torque Converter ClutchSystem Stuck OFF (Refer to Automatic Transaxle Diagnosis) | B | B | D
P0742 | Troque Converter Clutch System Stuck ON (Refer to Automatic Transaxle Diagnosis) | A | A | D
P0748 | Pressure Control Solenoid Valve Circuit Malfunction (Refer to Automatic Transaxle Diagnosis) | D | D | D
P0751 | Shift Solenoid 1 (1-2 Shift Solenoid) Performance/Stuck OFF (Refer to Automatic Transaxle Diagnosis) | A | A | D
P0753 | Shift Solenoid 1 (1-2 Shift Solenoid) Electrical (Refer to Automatic Transaxle Diagnosis) | A | A | D
P0756 | Shift Solenoid 2 (2-3 Shift Solenoid) Performance/Stuck OFF (Refer to Automatic Transaxle Diagnosis) | A | A | D
P0758 | Shift Solenoid 2 (2-3 Shift Solenoid) Electrical (Refer to Automatic Transaxle Diagnosis) | A | A | D
P1106 | Manifold Absolute Pressure (MAP) Sensor CKT Intermittent High Voltage | D | D | D
P1107 | Manifold Absolute Pressure (MAP) Sensor CKT Intermittent Low Voltage | D | D | D
P1111 | Intake Air Temperature (IAT) Sensor CKT Intermittent High Votlage | D | D | D
P1112 | Intake Air Temperature (IAT) Sensor CKT Intermittent Low Votlage | D | D | D
P1114 | Engine Coolant Temperature (ECT) Sensor CKT Intermittent Low Voltage | D | D | D
P1115 | Engine Coolant Temperature (ECT) Sensor CKT Intermittent High Voltage | D | D | D
P1121 | Throttle Position (TP) Sensor CKT Intermittent High Voltage | D | D | D
P1122 | Throttle Position (TP) Sensor CKT Intermittent Low Voltage | D | D | D
P1133 | HO2S Insufficient Switching Sensor 1 | B | D | --
P1134 | HO2S Transition Time Ratio Sensor 1 | B | D | --
P1336 | CKP System Variation Not Learned | A | D | --
P1351 | IC Circuit Open | B | B | B
P1352 | Bypass Cirucit Open | B | B | B
P1361 | IC Circuit Not Toggling | B | B | B
P1362 | Bypass Circuit Shorted | B | B | B
P1374 | 3X Reference Circuit | B | B | B
P1380 | EBCM DTC Rough Road Data Unusable | D | D | --
P1381 | Misfire Detected No EBCM/PCM Serial Data | B | B | --
P1404 | EGR Valve Stuck Open | B | D | --
P1441 | EVAP System Flow During Non-Purge | B | B | --
P1554 | Cruise Control Status Circuit | D | D | D
P1602 | EBCM/EBTCM Serial Data Circuit | D | D | D
P1610 | Standard Body Module Serial Data Circuit | D | D | D
P1626 | Theft Deterrent System Fuel Enable CKT | D | D | D
P1630 | Theft Deterrent PCM in Learn Mode | D | D | D
P1631 | Theft Deterrent Password Incorrect | D | D | D
P1635 | 5 Volt Reference (A) Circuit | B | B | B
P1639 | 5 Volt Reference (B) Circuit | D | D | D
P1641 | A/C Relay Control Circuit | D | D | D
P1651 | Fan 1 Relay Control Circuit | B | B | B
P1652 | Fan 2 Relay Control Circuit | B | B | B
P1662 | Cruise Control Inhibit Control Circuit | D | D | D
P1665 | EVAP Vent Valve Solenoid Control Circuit | B | B | --
P1671 | MIL Control Circuit | D | D | D
P1676 | EVAP Canister Purge Solenoid Control CKT | B | B | B
P1810 | Automatic Transmission Fluid Pressure Manual Valve Position Switch Malfunction (Refer to Automatic Transaxle Diagnosis) | B | B | D
P1811 | Maximum Adapt and Long Shift (Refer to Automatic Transaxle Diagnosis | D | D | D
P1860 | Torque Converter Clutch PWM Solenoid Circuit (Refer to Automatic Transaxle Diagnosis) | A | A | D
P1887 | TCC Release Switch Malfunction (Refer to Automatic Transaxle Diagnosis) | B | B | D