For 1990-2009 cars

# INSTALLATION PROCEDURE FOR RACK AND PINION STEERING GEARS

INSTALLATION PROCEDURE FOR CENTER-TAKE-OFF RACK AND PINION STEERING GEARS

#### VEHICLES AFFECTED: 1982-88 "J" CARS ----------------- 1986-88 "N" CARS When reinstalling a center-take-off rack and pinion steering gear in a 1982- 1988 "J" cars and 1986-1988 "N" Cars, always hand start the four clamp nuts then tighten the left side clamp nuts (driver's side of car) to the correct torque specifications first. Refer to Figure. The right side clamp nuts (passenger's side of car) should then be tightened to the correct torque specifications. Refer to Figure 1. The nut torque specification for 1982-1986 Models is: 38 N.m (28 lbs ft) The torque specification for 1987 and 1988 Models is: 30 N.m (22 lbs ft) This procedure will appear in the 1988 Chassis Service Manual steering gear installations. The procedure is applicable. to all current and past model center-take-off manual and power steering gear assemblies.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.