For 1990-2009 cars

# SMU - SEC. 3C - FRT. SUSPEN. SPECIFICATION REVISIONS

********************************************************************** SERVICE MANUAL UPDATE **********************************************************************

#### SUBJECT: SECTION 3C - FRONT SUSPENSION SPECIFICATION REVISIONS

#### MODELS: 1982-94 BUICK CENTURY 1982-90 CHEVROLET CELEBRITY 1982-94 OLDSMOBILE CUTLASS CIERA AND CRUISER 1982-91 PONTIAC 6000

THE FOLLOWING FRONT SUSPENSION SPECIFICATIONS HAVE BEEN REVISED FOR THE 1993 BUICK CENTURY AND OLDSMOBILE CUTLASS CIERA AND CRUISER:

FRONT SUSPENSION STRUT MOUNT NUT 22 N.M (16 LB.FT.) FRONT SUSPENSION STRUT NUT 85 N.M (63 LB.FT.)

THE FRONT SUSPENSION STEERING KNUCKLE NUT TIGHTENING SPECIFICATION FOR ALL 1982-94 A-CARS HAS BEEN REVISED TO A NEW SPECIFICATION OF 53 N.M (39 LB.FT.).

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.