For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Clean the dirt and foreign material from the brake hoses and fittings.
3. Remove the rear brake pipe (3) from the brake hose (1).
4. Remove the retainer clips (4) from the brake hose (3).
5. Remove the brake hose (3) from the bracket (1).
6. Remove the retaining bolt (3) from the rear brake hose (2).
7. Remove the brake hose (2) from the vehicle.

### Installation Procedure

1. Install the brake hose (2) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the retaining bolt (3) to the rear brake hose (2).

Tighten
Tighten the retaining bolt to 50 N·m (37 lb ft).

3. Install the brake hose (3) to the bracket (1).
4. Install the retainer clip (4) to the brake hose (1).
5. Install the rear brake pipe (3) to the brake hose (1).

Tighten
Tighten the fitting to 27 N·m (20 lb ft).

6. Bleed the brake hydraulic system. Refer to Hydraulic Brake System Bleeding .
7. Lower the vehicle.