For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38491 Spark Plug Heat Shield Removal Tool

1. Turn OFF the ignition switch.
2. Remove the spark plug wire retaining clips from the engine.
3. Rotate the engine.

Notice: Twist the spark plug boot one-half turn in order to release the boot. Pull on the spark plug boot only. Do not pull on the spark plug wire or the wire could be damaged.

Important: Transfer any of the following when replacing the spark plug wires:

• | Spark plug wire conduit

• | Spark plug wire retaining clips

4. Disconnect the spark plug wires from the spark plugs using the J 38491 . Be sure to note the position of the spark plug wires BEFORE removing the spark plug wires.

### Installation Procedure

1. Connect the spark plug wires (1) to the proper location. Refer to the callouts for the coil-to-cylinder combinations.
2. Return the engine to the proper position.
3. Install the spark plug wire (1) retaining clips to the engine.