For 1990-2009 cars

# FRONT STABILIZER BAR INSULATOR BUSHING SQUEAK

#### VEHICLES AFFECTED: 1985-86 'J' and 'N' models

A squawk noise from the front stabilizer bar insulator bushings may be corrected by installing new Teflon lined bushings. The new bushings are being used in production beginning approximately February 1, 1986.

Selection Chart for 1985-86 'J' and 'N' models shown below:

STABILIZER BAR NEW BUSHING SHAFT DIAMETER PART NUMBER -------------- ----------- 24 mm 22532210 26 mm 22532211 28 mm 22532212 30 mm 22532213

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.