For 1990-2009 cars

# WINDNOISE (POSSIBLE WATERLEAK) AT LOWER LEFT CORNER OF

#### SUBJECT: WINDNOISE (POSSIBLE WATERLEAK) AT LOWER LEFT CORNER OF WINDSHIELD (RESEAL WITH URETHANE ADHESIVE)

#### MODELS: 1995 BUICK CENTURY 1995 OLDSMOBILE CUTLASS CIERA

#### CONDITION:

SOME OF THE ABOVE LISTED VEHICLES MAY HAVE A WINDNOISE (AND POSSIBLE WATERLEAK) THAT MAY OCCUR AT THE LOWER LEFT CORNER OF THE WINDSHIELD.

#### CORRECTION:

THIS CONDITION MAY BE CORRECTED BY REMOVING THE WIPER ARMS AND COWL GRILLE AND RESEALING THE WINDSHIELD SEALING AREA WITH URETHANE ADHESIVE.

DO NOT REMOVE WINDSHIELD TO REPAIR THIS CONDITION!

#### IMPORTANT: IF A SUBLET REPAIR FACILITY IS BEING USED, THE SERVICE MANAGER SHOULD PROVIDE A COPY OF THIS BULLETIN TO THAT FACILITY.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C0020 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.