For 1990-2009 cars

# SPECIAL POLICY: EXTERIOR PAINT ADHESION TO LOWER BODY

#### MODELS/YEARS: 1986 OLDSMOBILE CALAIS

#### CONDITION

A durability feature on 1986 Oldsmobile Calais models is a chip resistant mataial applied to the lower portion of the car body, which is then covered by the car's paint finish. We have found that on some of these cars, the adhesion between the two materials may be inadequate. On the affected cars, this condition may result in flaking or chipping of the paint finish from these lower portions of the car's body.

#### VEHICLES INVOLVED

Involved are certain 1986 Oldsmobile Calais models within the following VIN breakpoints:

Plant Beginning Up To And Including ----- --------- ------------------- Lansing (M) GM363436 GM367252 Lansing (C) GC829107 GC829624

#### OWNER NOTIFICATION

Owners of vehicles involved in this Special Policy will be notified by Oldsmobile Division.

#### SPECIAL POLICY ADJUSTMENT

General Motors will refinish all areas of the lower portion of the vehicle body in which the chip resistant material was applied should those areas exhibit excessive chipping or flaking of the basecoat/clearcoat finish.

This Special Policy covers both materials and labor for a period of three (3) yeam from the date the vehicle was originally placed in service, regardless of mileage.

This "Special Policy Adjustment Bulletin" should be filed in the 3-ring binder furnished to the dealer by General Motors.

#### SERVICE PROCEDURE

1. Remove the basecoat/clearcoat from areas as shown in figure 1. In some cases the basecoat/clearcoat can be effectively removed by using an air hose to blow it away from the chip resistant material.

#### NOTE: Every effort should be made to leave as much of the chip resistant material as possible. Therefore, removal of the basecoat/clearcoat by sanding should be done very carefully using 400 paper and finishing with 600 paper.

2. Refinish areas by using recommended basecoat/clearcoat application procedures specified for the materials being used.

The following materials or their equivalent are recommended:

Centari Basecoats Centari Basemaker - 82805 Centari 780S Clearcoat Centari 782S Catalyst

Lacquer materials may also be used for this repair where local conditions require it.

#### WARRANTY CLAIM INFORMATION

Trouble Labor Material Labor Operation Code Operation Allowance Hours* --------- ------- --------- --------- -----

Refinish Areas as 92 T4250 22.86 2.2 Shown in Figure 1

*Includes paint mix time and rocker panel molding R & R.

When submitting for credit via DCS, the Line Total amount is automatically calculated using your mechanical labor rate. Since this is a paint repair and should be computed at body labor rates, it will be necessary to use the special override feature to adjust the line total to reflect your body rate. Refer to vendor instruction.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.