For 1990-2009 cars

# V6 DIESEL FLYWHEEL TORQUE CORRECTION 82 SERVICE MANUAL

IN THE 1982 SERVICE MANUAL ON PAGE 6A6-42 THE FLYWHEEL TO CRANKSHAFT TORQUE IS INCORRECT. THE CORRECT FLYWHEEL TO CRANKSHAFT TORQUE IS 90 N.M (65 FT. LBS.). NOTE THIS CORRECTION IN YOUR SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.