For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the door handle bezel. Refer to Door Handle Bezel Replacement .
3. Remove the power door lock switch (2) from the door handle bezel (3) by prying the power door lock switch from the retainers.
4. Disconnect the electrical connector (1) from the power door lock switch (2) .

### Installation Procedure

1. Install the power door lock switch (1) to the door handle bezel (3).
2. Connect the electrical connector (1) to the power door lock switch (2).
3. Install the door handle bezel. Refer to Door Handle Bezel Replacement .
4. Connect the negative battery cable.