For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 0B COOLING SYSTEM CAPACITIES

#### MODELS/YEARS 1989-90 CUTLASS CALAIS MODELS

What follows is corrected engine cooling system coolant capacities for the 1989 and 1990 Cutlass Calais.

2.3L (VIN D) All 9.8 Liters (10.4 Ouarts) 2.3L (Vin A) All 9.8 Liters (10.4 Quarts)

2.5L (VIN U) All 1 0. 1 Liters (10.7 Quarts)

3.3L (VIN N) All 12.0 Liters (12.7 Quarts)

Please mark a reference to this bulletin in your copy of the following service manuals in Section OB, Maintenance and Lubrication, at the "Approximately Fluid Capacities" Chart:

1989 Cutlass Calais, Page OB-9 1990 Cutlass Calais, Page OB-9

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.