For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the door outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .
3. Remove the door inner belt sealing strip. Refer to Inner Belt Sealing Strip Replacement .
4. Remove the door window frame applique. Refer to Door Frame Applique Replacement .
5. Remove the door water deflector. Refer to Door Water Deflector Replacement .
6. Remove the rear side door window. Refer to Rear Side Door Window Replacement .
7. Remove the screw securing the rubber seal strip to the upper window frame.
8. Remove the rubber seal strip from the upper window frame.
9. Remove the screws (2,4) securing the rear door stationary window to the inner door panel.
10. Remove the bolt (3) securing the rear door stationary window to the inner door panel.
11. Remove the rear door stationary window (1).

### Installation Procedure

1. Install the rear door stationary window (1).
2. Install the rubber seal strip to the upper window frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screw securing the rubber seal strip to the upper window frame.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the screws (2,4) securing the rear door stationary window to the inner door panel.

Tighten
Tighten the screw to 2 N·m (18 lb in).

5. Install the bolt (3) securing the rear door stationary window to the inner door panel.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

6. Install the rear side door window. Refer to Rear Side Door Window Replacement .
7. Install the door water deflector. Refer to Door Water Deflector Replacement .
8. Install the door window frame applique. Refer to Door Frame Applique Replacement .
9. Install the door inner belt sealing strip. Refer to Inner Belt Sealing Strip Replacement .
10. Install the door outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .
11. Install the door trim panel. Refer to Door Trim Panel Replacement .