For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the door power window switch (3) from the door by prying at the top of the switch with a flat bladed tool.
3. Disconnect the electrical connector (2) from the power door window switch.
4. Remove the bezel (1) from the power door window switch (3) by prying out the retainers (4) with the flat bladed tool.

### Installation Procedure

1. Install the bezel (1) to the door power window switch (3).
2. Connect the electrical connector (2) to the power window switch (3).
3. Install the power window switch (3) to the door.
4. Connect the negative battery cable.