For 1990-2009 cars

# COLD AIR LEAK AT PASSENGER FOOT AREA (INSTALL CAULK)

COLD AIR LEAKING ON PASSENGER FOOT AREA

#### VEHICLES AFFECTED: 1986-1987 J AND N CARLINES WITH OPTION C60 ----------------- Revised to correct a call-out in the artwork

Some 1986 and 1987 "J" and "N" car owners may comment on a condition where cold air may be blowing into the passenger foot area. The air leak has been identified as coming from the joint between the heater core cover and evaporator case and generally located toward the front of the vehicle where the AC module meets the front of dash. The leaks could be found on either side of module. (See Figure)

This condition may be repaired by applying 3M strip caulk (or equivalent) to the case joint area where air leakage is found.

#### Warranty Information:

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.