For 1990-2009 cars

# CYLINDER HEAD BOLT LENGTH SERVICE INFORMATION

#### VEHICLES AFFECTED: 1985 'N' Series Equipped with 3.0L V-6 (VIN Code L) Engines ----------------------------------

There are three different length head bolts used on the above 3.0L engine. Head bolt length by location is shown below.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.