For 1990-2009 cars

### Removal Procedure

1. Raise the door window to the full up position.
2. Remove the door trim panel. Refer to Door Trim Panel Replacement .
3. Remove enough of the door water deflector in order to access the rear door inside handle. Refer to Door Water Deflector Replacement .
4. Remove the screws (2) securing the rear door lock (1).
5. Remove the rear door inside handle screw (2).
6. Remove the door inside handle rod (2) from the rear door inside handle (3).
7. Remove the door inside locking rod (4) from the rear door inside handle (3).
8. Remove the rear door inside handle (3).

### Installation Procedure

1. Install the door inside handle rod (2) to the rear door inside handle (3).
2. Install the door inside locking rod (4) from the rear door inside handle (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rear door inside handle screw (2).

Tighten
Tighten the screw to 1 N·m (9 lb in).

4. Install the rear door lock screws (2).

Tighten
Tighten the screw to 6 N·m (53 lb in).

5. Install the door water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Door Trim Panel Replacement .