For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the front wheelhouse panel splash shield retainers (2).
4. Remove the front wheelhouse panel splash shield bolts (3).
5. Remove the front wheelhouse panel splash shield (4).

### Installation Procedure

1. Install the front wheelhouse panel splash shield (4).
2. Install the front wheelhouse panel splash shield bolts (3).
3. Install the front wheelhouse panel splash shield retainers (2).
4. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
5. Lower the vehicle.