For 1990-2009 cars

# Warranty Admin. - January 1, 2001 Labor Time Guide Updates

Subject: | January 1, 2001 Labor Time Guide Updates

Models: | 1996-2002 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

#### LTG Update - C Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ADJUSTER ASSEMBLY, FRONT SEAT POWER - R&R OR REPLACE

- NOTE: No Change to "PART GP" or Labor Operations C6040 or C6041

SPLIT/DIVIDED SEAT PASSENGER |  | C6050 |  |  |  |  |  |

- ONE SIDE

R

0.7

2.3

2.3

2.3

2.3

2.3

SPLIT/DIVIDED SEAT DRIVER |  | C6051 |  |  |  |  |  |

- ONE SIDE

R

0.7

2.3

2.3

2.3

2.3

2.3

- NOTE: No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MANIFOLD OR GASKET, INTAKE - REPLACE

- NOTE: Applies to V8 Engine, Code G

MANIFOLD | N | J0250 | -- | -- | -- | -- | -- | 1.7

- POLICY: E (7/70 California - Includes other applicable states)

GASKET | N | J0251 | -- | -- | -- | -- | -- | 1.3

- POLICY: E

ADD: |  |  |  |  |  |  |  |

- A- With A/C

N

--

--

--

--

--

0.5

*IND: N - New/R - Revised

#### LTG Update - C/K - New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
97 | 98 | 99 | 00 | 01 | 02
YEAR VIN CODE
V | W | X | Y | 1 | 2
HEADLINING ASSEMBLY - R&R OR REPLACE

- NOTE: No Change to "PART GP", "POLICY" or Labor Operations C3122 or C3123

ONE PIECE |  | C3128 |  |  |  |  |  |

- YUKON/TAHOE

--

--

--

1.8

1.8

1.8

- SUBURBAN/YUKON XL

--

--

--

1.8

1.8

1.8

- CONV CAB

R

--

--

3.3

3.3

3.3

3.3

- CLUB/EXTENDED CAB

R

--

--

3.5

3.5

3.5

3.5

- No Change to "ADD" Condition

ACTUATOR AND/OR ASSEMBLY, LUMBAR - REPLACE |  |  |  |  |  |  |  |
RIGHT | N | C6627 | -- | -- | 1.0 | 1.0 | 1.0 | 1.0
LEFT | N | C6628 | -- | -- | 1.0 | 1.0 | 1.0 | 1.0
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

0-0.3

0-0.3

0-0.3

0-0.3

- B- With Side Impact Air Bags

N

--

--

--

0.3

0.3

0.3

BELT, SAFETY FRONT (RETRACTOR SIDE) - R&R OR REPLACE

- PART GP: 14.875

- INC: Enable and Disable SIR System (Utility only)

RIGHT | R | C9040 |  |  |  |  |  |

- PICKUP

- BENCH

--

--

0.5

0.5

0.5

0.5

- BUCKET

--

--

0.6

0.6

0.6

0.6

- UTILITY

--

--

--

0.9

0.9

0.9

LEFT | R | C9041 |  |  |  |  |  |

- PICKUP

- BENCH

--

--

0.5

0.5

0.5

0.5

- BUCKET

--

--

0.6

0.6

0.6

0.6

- UTILITY

--

--

--

0.9

0.9

0.9

SENSOR, YAW RATE - REPLACE | N | H2582 | -- | -- | -- | -- | -- | 0.3
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

0-0.3

GASKET, TRANSFER CASE TO ADAPTER - REPLACE | R | K4250 | -- | -- | 1.4 | 1.4 | 1.4 | 1.4
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

--

--

0-0.3

0-0.3

0-0.3

0-0.3

CLOCK ASSEMBLY - REPLACE |  |  |  |  |  |  |  |

- ESCALADE

N

N4210

--

--

--

--

--

0.2

HEAD, REAR COMPARTMENT AUDIO CONTROL - REPLACE | N | R0862 | -- | -- | -- | -- | -- | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

--

0-0.3

CELLULAR MOBILE TELEPHONE SYSTEM COMPONENTS - R&R OR REPLACE

- NOTE: No Change to "POLICY" or Labor Operations R5110 thru R5139 and R5144

VEHICLE INTERFACE UNIT (ON-STAR) | R | R5140 | -- | -- | 0.8 | 0.8 | 0.8 | 0.8

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - E Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PLUG, EXPANSION - REPLACE

- NOTE: Time(s) for removal of necessary components to gain access to plug must be submitted as "Other Labor Hours", and have appropriate authorization.

- NOTE: Applies to V8 Engine, Codes 9 and Y

N

J1600

0.3

0.3

0.3

0.3

0.3

0.3

*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | R | J6441 | 0.2 | 0.2 | 0.6 | 0.6 | 0.6 | 0.6
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

SEAL, FUEL SENDER/PUMP ASSEMBLY (TANK UNIT) - REPLACE

- POLICY: E

L1195

1.2

1.2

1.2

1.2

1.2

1.2

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
HEADREST AND/OR COVER, FRONT SEAT - R&R OR REPLACE

- NOTE: No Change to "POLICY"

PASSENGER |  | C6690 | 0.3 | 0.2 | 0.3 | 0.3 | 0.3 | 0.3
DRIVER |  | C6691 | 0.3 | 0.2 | 0.3 | 0.3 | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- NOTE: No Change to "ADD" Conditions A or B

- C- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

PLUG, EXPANSION - REPLACE

- NOTE: Time(s) for removal of necessary components to gain access to plug must be submitted as "Other Labor Hours", and have appropriate authorization.

- NOTE: Applies to V8 Engine, Codes 9 and Y

N

J1600

0.3

0.3

0.3

0.3

0.3

0.3

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
97 | 98 | 99 | 00 | 01 | 02
YEAR VIN CODE
V | W | X | Y | 1 | 2
PLUG, EXPANSION - REPLACE

- NOTE: Time(s) for removal of necessary components to gain access to plug must be submitted as "Other Labor Hours", and have appropriate authorization.

- NOTE: Applies to V8 Engine, Codes 9 and Y

N

J1600

0.3

0.3

0.3

0.3

0.3

0.3

SENSOR, OXYGEN (CATALYST MONITORING) - REPLACE |  | J6380 |  |  |  |  |  |

- FRONT

0.2

0.2

- REAR

R

0.3

0.3

0.3

0.3

0.3

0.3

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CONSOLE, ROOF - R&R OR REPLACE

- PART GP: 10.225

R

C2870

0.4

0.4

0.4

0.4

0.4

0.4

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CORE, EVAPORATOR - REPLACE |  | D3320 |  |  |  |  |  |

- MALIBU & CUTLASS

--

1.3

1.3

1.3

1.3

1.3

- GRAND AM

R

2.1

2.1

2.1

4.9

4.9

4.9

- ACHIEVA - 4 CYL

R

2.1

2.1

4.8

- ACHIEVA - 6 CYL

R

2.1

2.1

4.8

- ALERO

R

--

--

--

4.8

4.8

4.8

- SKYLARK - 4 CYL

2.1

2.1

2.1

- SKYLARK - 6 CYL

2.1

2.1

2.1

- No Change to "ADD" Condition

BEARING AND HUB ASSEMBLY, FRONT WHEEL - REPLACE

- NOTE: No Change to Labor Operation E2327

RIGHT |  | E2320 |  |  |  |  |  |

- MALIBU & CUTLASS

--

0.8

0.8

0.8

0.8

0.8

- ACHIEVA & SKYLARK

0.7

0.7

0.7

- GRAND AM & ALERO

R

0.7

0.7

0.7

0.7

0.7

0.7

LEFT |  | E2321 |  |  |  |  |  |

- MALIBU & CUTLASS

--

0.8

0.8

0.8

0.8

0.8

- ACHIEVA & SKYLARK

0.7

0.7

0.7

- GRAND AM & ALERO

R

0.7

0.7

0.7

0.7

0.7

0.7

- No Change to "ADD" Conditions

FILTER, FUEL (IN-TANK STRAINER) - REPLACE | N | L1198 | -- | -- | -- | 1.2 | 1.2 | 1.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

0-0.3

0-0.3

0-0.3

RECEIVER, REMOTE DOOR/REAR COMPARTMENT LOCK - REPLACE

- NOTE: No Change to "PART GP" or "INC"

R

R4480

0.3

0.3

0.3

0.3

0.3

0.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

R

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SENSOR, FUEL TANK VACUUM - REPLACE | R | L0622 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
HOOK, COAT - R&R OR REPLACE

- NOTE: No Change to "PART GP" or "INC"

R

C3140

0.2

0.2

0.2

0.2

0.2

0.2

ADD: |  |  |  |  |  |  |  |

- A- To Color Coat

R

0.4

0.4

0.4

0.4

0.4

0.4

|  |  | GB | GB | GB | GB | GB | GB
*IND: N - New/R - Revised

#### LTG Update - V Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
LINK AND/OR LINK BUSHINGS OR BUSHING AND/OR BRACKET, FRONT STABILIZER SHAFT AT CONTROL ARM - R&R OR REPLACE

- NOTE: No Change to "PART GP" or "NOTE"

- RIGHT

R

E2140

--

0.4

0.4

0.4

0.4

0.4

- LEFT

R

E2141

--

0.4

0.4

0.4

0.4

0.4

- BOTH

R

E2147

--

0.6

0.6

0.6

0.6

0.6

CYLINDER, IGNITION LOCK - R&R OR REPLACE

- NOTE: No Change to "PART GP" or "INC"

R

E7200

--

0.8

0.8

0.8

0.8

0.8

CONTROL ASSEMBLY, FLOOR SHIFT - REPLACE

- INC: Adjust

K5225

- MALIBU & CUTLASS

R

--

1.1

1.1

1.1

0.6

0.6

- ACHIEVA & SKYLARK

0.4

0.4

0.4

- GRAND AM & ALERO

0.4

0.4

0.4

0.7

0.7

0.7

CABLES, BATTERY - REPLACE

- NOTE: No Change to "PART GP" or Labor Operation N0126

- POSITIVE

- BATTERY TO STARTER

R

N0120

--

1.3

1.3

1.3

1.3

1.3

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
TUBE, OIL LEVEL INDICATOR - REPLACE

- NOTE: Applies to V6 Engine, Codes X and H

R

J0930

20

2.0

--

0.6

0.6

0.6

*IND: N - New/R - Revised