For 1990-2009 cars

#### Tools Required

J 41228 Output Shaft Sleeve Installer

1. Inspect the output shaft (94) for damage to the splines, snap ring grooves and the journals.
2. Clean and dry the output shaft.

Important: You must use the J 41228 in order to install the sleeve onto the output and stub shafts. If you do not use the J 41228 , you will cause a fluid leak.

3. Place a sleeve (56) over the end of the output shaft (94).
4. Install the collet into the output shaft snap ring groove with the collet attached to the threaded collet shaft.
5. Place the sleeve installing tube over the collet. Be sure the small outside diameter of the tube fits securely into the sleeve.
6. Install the bearing and nut onto the threaded collet shaft.
7. in order to move the installing tube and press the sleeve onto the output shaft, hold the end of the threaded collet shaft while tightening the nut down.
8. Remove the J 41228 .