For 1990-2009 cars

Problem | Action
--- | ---
The front or rear stabilizer shaft is loose. |

1. Inspect the mounting bolts and links.
2. Torque to proper specifications.

Refer to Stabilizer Shaft Replacement in Front Suspension or Stabilizer Shaft Replacement in Rear Suspension.

The front or rear struts are worn. | Inspect and service as required. Refer to Strut Assembly Replacement in Front Suspension or Strut Assembly Replacement in Rear Suspension.
The vehicle is overloaded. | Reduce the load.
The tire pressure(s) is incorrect. | Inflate the tire(s) to proper specifications. Refer to Tire Description in Maintenance and Lubrication.