For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Seat Replacement in Seats.
2. Fold the console compartment up.
3. Remove the console trim plate. Refer to Console Trim Plate Replacement .
4. Remove the rear cupholder (1).
5. Remove the screws.
6. Remove the console (2).

### Installation Procedure

1. Install the console (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the rear cupholder (1).
4. Install the console trim plate. Refer to Console Trim Plate Replacement .
5. Install the console compartment.
6. Install the front seats. Refer to Seat Replacement in Seats.