For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable
2. Remove the transmission assembly from the vehicle. Refer to Transmission Replacement .
3. Remove the torque converter assembly (55) from the transmission.
4. Remove the turbine shaft O-ring (41) on the end of the turbine shaft using a screwdriver.

### Installation Procedure

1. Assemble a new turbine shaft O-ring (41) on the end of the turbine shaft.
2. Install the torque converter (55) onto the transmission.
3. Install the transmission into the vehicle. Refer to Transmission Replacement .
4. Connect the negative battery cable.
5. Adjust the oil level. Refer to Transmission Fluid Check .