For 1990-2009 cars

Problem | Action
--- | ---
Foreign material obstructing the turn signal | Clean inspect and replace the components as necessary. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
Loose or distorted springs | Replace the components as necessary. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
A loose switch arm | Tighten the arm to specifications. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .
Loose switch mounting screws |

1. Inspect the following components:

• | The switch installation

• | The mounting screw bosses on the lock housing cover.

2. Replace the components as necessary.

Refer to Multifunction Turn Signal Lever Replacement - On Vehicle .