For 1990-2009 cars

### Removal Procedure

1. Remove the washer solvent from the washer solvent container.
2. Disconnect the electrical connectors from the washer pump and the solvent level sensor switch.
3. Disconnect the hose from the washer pump.
4. Loosen the nut at the bottom of the washer solvent container.
5. Remove two nuts and the washer solvent container.
6. Remove the washer pump and seal from the container.
7. Remove the solvent level sensor switch and seal from the washer solvent container.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: The tab on the solvent level sensor switch must be lined up with the slot in the hole.

1. Install the solvent level sensor switch and seal in the washer solvent container.

Important: The new washer pump must be pushed all the way into the container seal.

2. Install the washer pump and the seal into the washer solvent container.
3. Install the washer solvent container with three nuts.

Tighten
Tighten the nuts to 5 N·m (44 lb in).

4. Connect the electrical connectors to the solvent level sensor switch and the washer pump.
5. Connect the hose to the washer pump.
6. Fill the washer solvent container with washer solvent.