For 1990-2009 cars

### Removal Procedure

1. Open the jack storage container (1).
2. Remove the bolts (2) that retain the container to the body.
3. Remove the jack storage container (1).

### Installation Procedure

1. Install the jack storage container (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (2) in order to retain the container (1) to the body.

Tighten
Tighten the bolts to 13.5 N·m (119 lb in).

3. Close the jack storage container (1).