For 1990-2009 cars

Caution: Always use double walled steel brake pipe when replacing brake pipes. The use of any other pipe is not recommended and may cause brake system failure. Carefully route and retain replacement brake pipes. Always use the correct fasteners and the original location for replacement brake pipes. Failure to properly route and retain brake pipes may cause damage to the brake pipes and cause brake system failure.

#### Tools Required

J 29803-A ISO Flaring Tool

Important: This vehicle uses only ISO flares on the brake pipe connections. Do not attempt to use single or double lap flares when replacing the brake pipes.