For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC/6E3 DIAG. CHART DTC-58(PASS-KEY)

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3 - DIAGNOSTIC CHART DTC 58 (PASS KEY II)

#### VEHICLES AFFECTED: 1993 "C" AND "H" MODELS WITH 3800 ENGINE (VIN L)

This bulletin updates service manual Section 6E3 for C/H carlines equipped with 3800 (VIN L) engines. The DTC 58 PASS-key II fuel enable circuit diagnostic chart was inadvertently omitted from the VIN L section of the service manual. To diagnose a DTC 58, use the diagnostics found on pages 6E3-A-100 and 6E3-A-101 of the 3800 (VIN 1) section of the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.