For 1990-2009 cars

### Removal Procedure

1. Carefully disengage the retainers on the back side of the molding (1).
2. Pull outward on the garnish molding.
3. Remove the windshield pillar garnish molding (1).

### Installation Procedure

1. Connect the new retainers (2) to the windshield pillar garnish molding (1) if they are broken or damaged.
2. Align the retainers (2) to the holes in the windshield pillar.
3. Press the windshield pillar garnish molding (1) in order to secure.