For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the lamp housing. Insert a flat bladed tool under the forward edge of the housing to depress the retaining clip.
3. Disconnect the electrical connector.
4. Remove the bulbs as necessary. Pliers may be needed in order to rotate the bulbs out of the housing.

### Installation Procedure

1. Install the bulb holders and/or bulbs.
2. Connect the electrical connector.
3. Snap the door lamp housing into the trim panel.
4. Connect the negative battery cable.