For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: This test checks the condition of the height sensor and the height sensor supply and ground circuits.
1 |

1. Disconnect the height sensor connector.
2. Measure the voltage from the height sensor connector (vehicle side), terminal C to ground.

Is battery voltage measured?

Battery Voltage

Go to Step 3

Go to Step 2

2 | Repair the open circuit condition:

• | Vehicles w/optional inflator valve - Repair the open circuit condition in one of the following circuits/components

• | CKT 1042 (RED) from the height sensor to connector C440, terminal D

• | CKT 1246 (LT BLU) from connector C440, terminal D, to the inflator timer-relay

• | Inflator timer-relay terminal B to terminal D (replace if no continuity)

• | CKT 1042 (RED) from the inflator timer-relay to the ELC fuse in the RH MaxiFuse® Block

• | Vehicles w/o optional inflator valve - Repair the open circuit condition in CKT 1042 (RED) between the height sensor and the ELC fuse in the RH MaxiFuse® Block.

Is the repair or replacement complete?

--

Go to Automatic Level Control System Operation Check

--

3 | Measure the voltage from the height sensor connector (vehicle side), terminal C to the same connector, terminal A. Is battery voltage measured? | Battery Voltage | Go to Step 5 | Go to Step 4
4 | Repair the open circuit condition in CKT 1250 (BLK). Is the repair complete? | -- | Go to Automatic Level Control System Operation Check | --
5 |

1. Turn the ignition switch to the ON position.
2. Measure the voltage from the height sensor connector (vehicle side), terminal D to the same connector, terminal A.

Is battery voltage measured?

Battery Voltage

Go to Step 7

Go to Step 6

6 | Repair the open circuit condition in CKT 641 (BRN). Is the repair complete? | -- | Go to Automatic Level Control System Operation Check | --
7 |

1. Check the height sensor connector for proper terminal contact.
2. Cycle ignition switch and return ignition switch to ON.

Does the air compressor operate for 3 to 5 seconds after an initial 35 to 55 second delay?

--

Go to Step 9

Go to Step 8

8 | Replace the height sensor. Refer to Automatic Level Control Sensor and Bracket Replacement . Is the replacement complete? | -- | Go to Automatic Level Control System Operation Check | --
9 |

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information. NOTE: The vehicle must be raised on a drive-on lift or be supported at the rear under the rear axle. Full vehicle weight must be on the rear axle.
2. Disconnect the link from the position sensor.
3. Move the height sensor arm up so that it is approximately 45 degrees above level (to the floor).

Does the air compressor run after the 17 to 27 second delay?

--

Go to Step 11

Go to Step 10

10 | Replace the height sensor. Refer to Automatic Level Control Sensor and Bracket Replacement . Is the replacement complete? | -- | Go to Automatic Level Control System Operation Check | --
11 | Move the height sensor down slowly until the air compressor stops. Does the air compressor stop? | -- | Go to Step 13 | Go to Step 12
12 | Replace the height sensor. Refer to Automatic Level Control Sensor and Bracket Replacement . Is the replacement complete? | -- | Go to Automatic Level Control System Operation Check | --
13 | Move the height sensor arm down so that it is approximately 45 degrees below level (to the floor). After a 17 to 27 second delay, does air escape from the air compressor as the vehicle begins to lower? | -- | Go to Step 15 | Go to Step 14
14 | Replace the height sensor. Refer to Automatic Level Control Sensor and Bracket Replacement . Is the replacement complete? | -- | Go to Automatic Level Control System Operation Check | --
15 | Adjust the height sensor. Refer to Automatic Level Control Sensor Adjustment . Is the adjustment complete? | -- | Go to Automatic Level Control System Operation Check | --