For 1990-2009 cars

### Removal Procedure

1. Remove the glass panel (3). Refer to Sunroof Glass Panel Replacement .
2. Pull the seal away from the channel at the rim of the glass in order to remove the seal (1).

### Installation Procedure

1. Clean the old adhesive from the channel at the rim of the glass.
2. Apply a 152 mm (6 in) strip of adhesive to the side of the glass panel (3).
3. Start with the end of the weather-strip (1) covering 77 mm (3.03 in) of the previously applied adhesive.

Working around the glass panel (3), push the weather-strip (1) into the channel.

4. Cut free the end of the weather-strip (1) at the side in order to allow a 3-5 mm (1/8-3/16 in) overlap.
5. Place a small amount of the adhesive on the free end of the weather-strip (1).
6. Butt the ends of the weather-strip (1) together, pushing the free end into the channel.
7. Force the remainder of the weather-strip (1) into the channel.
8. Allow the adhesive to dry.
9. Install the glass panel. Refer to Sunroof Glass Panel Replacement .
10. Adjust the glass panel in order to achieve good sealing action.