For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Lower the glass 3 cm (1 in).
4. Disconnect the electrical connectors.
5. Remove the speaker panel.
6. Remove the wiring harness retainers.
7. Tape the glass to the header.
8. Remove the nuts from the window sash.
9. Remove the front window channel. Refer to Front Side Door Window Channel Replacement .
10. Disconnect the rod from the outside door handle.
11. Disconnect the rod from the lock cylinder.
12. Remove the three door lock fasteners.
13. Remove the fasteners from the door module.
14. Remove the door module (3) with the lock attached.

### Installation Procedure

1. Install the door module (3) with the lock attached.
2. Install the fasteners to the door module in order to secure.
3. Instal the fasteners to the door lock.
4. Connect the rod to the lock cylinder.
5. Connect the rod to the outside door handle.
6. Install the fasteners to the window sash.
7. Install the front window channel. Refer to Front Side Door Window Channel Replacement .
8. Remove the tape from the glass.
9. Install the wiring harness retainers.
10. Install the speaker panel.
11. Connect the electrical connectors.
12. Adjust the window. Refer to Front Side Door Window Adjustment .
13. Install the water deflector. Refer to Door Water Deflector Replacement .
14. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .