For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire RAP System Check performed? | -- | Go to Step 2 | Go to Retained Accessory Power (RAP) System Check
2 |

• | Turn the ignition switch to the RUN position.

• | Close all of the doors.

• | Measure the voltage from the RAP relay terminal 87 (RH IP fuse block) to ground.

Is the voltage within the specified range?

10-15 V

Go to Step 3

Go to Step 4

3 | Measure the voltage from the RAP relay terminal 85 to ground. Is the voltage within the specified range? | 10-15 V | Go to Step 5 | Go to Step 6
4 | Repair the open or short to ground in CKT 1342 (RED). Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
5 | Measure the voltage from the RAP relay terminal 87A to ground. Is the voltage within the specified range? | 10-15 V | Go to Step 7 | Go to Step 8
6 | Repair the open or short to voltage in CKT 1540 (ORN) . Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
7 |

• | Close the doors.

• | Turn the ignition switch to OFF.

• | Cycle the ignition switch from RUN to OFF.

• | Measure the voltage from the RAP relay terminals 85 to 86.

Is battery voltage present for approximately 10 minutes?

--

Go to Step 11

Go to Step 14

8 |

• | Test CKT 4 (BRN) and CKT 1342 (RED) for an open or a short to ground.

• | Ensure that C202 terminals C6 and D5 are clean and tight.

Are the circuits OK?

--

Go to Step 9

Go to Step 10

9 | Replace the ignition switch. Refer to Steering Wheel and Column. Is the repair complete? |  | Go to Retained Accessory Power (RAP) System Check | --
10 | Repair the faulty circuit. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
11 | Ensure that the RAP relay terminals are clean and tight. Are the terminals OK? | -- | Go to Step 12 | Go to Step 13
12 | Replace the RAP relay. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
13 | Clean or repair the RAP relay terminals. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
14 |

• | Turn the ignition switch to RUN.

• | Disconnect the remote function actuator (RFA) connector.

• | Measure the voltage from the RFA connector terminal F15 to ground.

Is the voltage within the specified range?

10-15 V

Go to Step 15

Go to Step 16

15 | Measure the voltage from the RFA module connector terminals F15 to terminal F16. Is the voltage within the specified range? | 10-15 V | Go to Step 17 | Go to Step 18
16 | Repair open or short to ground in CKT 143 (YEL). Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
17 | Measure the voltage from the RFA module connector terminals E16 to F16. Is the voltage within the specified range? | 10-15 V | Go to Step 19 | Go to Step 20
18 | Repair the open or short to ground in CKT 1250 (BLK). Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
19 | Measure the voltage from RFA module connector terminals E15 to F16. Is the voltage within the specified range? | 10-15 V | Go to Step 21 | Go to Step 22
20 | Repair the open or short to ground in CKT 1540 (ORN). Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
21 |

• | Disconnect the RFA module connector.

• | Close all of the doors.

• | Measure the resistance from the RFA module connector terminals E10 and E12 to terminal F16.

Is the value within the specified range?

Infinite

Go to Step 23

Go to Step 26

22 | Repair CKT 39 (PNK) wiring for an open or a short to ground. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
23 | Ensure that the RFA terminals are clean and tight. Are the terminals OK? | -- | Go to Step 24 | Go to Step 25
24 | Replace the RFA module. Refer to Remote Control Door Lock Receiver Replacement . Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
25 | Clean or repair the RFA terminals. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --
26 | Repair the short to ground in CKT 49 (DK BLU), CKT 727 (DK BLU/WHT) or the door switches. Is the repair complete? | -- | Go to Retained Accessory Power (RAP) System Check | --