For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Place the seat upside down on a clean protected surface.
3. Remove the adjuster to seat cushion frame bolts (2).
4. Remove the adjuster assembly (4).

### Installation Procedure

1. Install the seat adjuster assembly (4) to the seat cushion frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat adjuster bolts (2).

Tighten
Tighten the bolts to 24 N·m (17 lb ft).

3. Install the front seat. Refer to Seat Replacement .