For 1990-2009 cars

### Removal Procedure

1. Remove the I/P sound insulators, as needed for access.
2. Remove the lower switch, twist counterclockwise to unlock and pull out of the retainer.
3. Remove the electrical connectors from the switch.

### Installation Procedure

1. Slide the switch (with all the connections made) into the retainer.
2. Press the switch in until the switch plunger is fully depressed into the switch barrel.
3. Twist the switch clockwise until the travel stop has been reached (approximately 60 degrees). With the switch fully locked, the electrical connector will face the 3 o'clock position.