For 1990-2009 cars

# ABS/TCS FAULT CODES 43/47 MISLABELED - SHOULD BE 44/48

#### SUBJECT ABS/TCS FAULT CODES 43 AND 47 HAVE BEEN MISLABELED AND SHOULD BE 44 AND 48

#### MODELS/YEARS 1992 EIGHTY EIGHT AND NINETY EIGHT ----------------------------------------------------------------------------

Due to a fault code labeling error in the electronic brake control module software in 1992 Eighty Eight and Ninety Eight models, ABS/TCS fault codes 44 and 48 have been mislabeled as fault codes 43 and 47, respectively. Codes 43 and 47 should simply be treated as codes 44 and 48 when diagnosing a vehicle. The diagnostics in Section 5El of the service manual reflect the correct notation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.