For 1990-2009 cars

### Removal Procedure

1. Lower the window all the way down.
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Starting at one end of the window inner belt molding, pull upward to release the molding.

### Installation Procedure

1. Position the door window inner belt molding over the flange of the door inner panel.
2. Press down, being careful not to distort the molding, in order to engage the door window inner belt molding the entire length of the door.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .