For 1990-2009 cars

# ENGINE OIL RECOMMENDATIONS PREFERRED VISCOSITIES

#### Models/Years All Oldsmobile Models

The purpose of this bulletin is to:

- Advise you of the reasons for changes in engine oil viscosity recommendations, and

- Explain the new API service symbol which should assist vehicle owners in finding engine oils recommended for engines in Oldsmobile models.

#### Gasoline Engine Oil Viscosity Recommendations

Since 1980, the preferred viscosities for gasoline engines in Oldsmobile models are SAE 10W-30 for the larger engines and SAE 5W-30 for the smaller engines (engine sizes defined later).

SAE 10W40 is not included in the viscosity chart for 1984 gasoline engines for several reasons, including:

- Fuel economy with SAE 10W-30 oils is about 1 percent better than that with SAE 10W40 oils.

- SAE 10W-30 oils generally produce less piston and ring deposits than SAE 10W40 oils. Such deposits can lead to stuck rings and increased oil consumption.

The use of SAE 10W-40 engine oil in a vehicle equipped with a gasoline engine will not automatically void the General Motors Corporation New Car Limited Warranty. However, since SAE 10W-40 engine oil is not recommended for use in 1984 Oldsmobile vehicles equipped with gasoline engines, if the use of such oil CAUSES DAMAGE, the cost of the engine repair will not be covered by the warranty. The Warranty does not cover any damage due to the use of non-recommended oil, whether SAE 10W-40 or some other viscosity. In addition, the Warranty does not cover damage caused by the use of oils that do not meet the recommended API quality or SAE viscosity grade.

#### Diesel Engine Oil Viscosity Recommendations

Preferred viscosity for diesel engines in Oldsmobile passenger cars is SAE 30.

SAE 10W-40 oils have never been recommended for diesel engines in Oldsmobile passenger cars. Nevertheless, some owners have used SAE 10W-40 oils and, in dome cases, experienced engine damage caused by excessive piston and ring deposits. In an effort to clarify the Oldsmobile recommendations for passenger cars, the 1984 owner's manuals state specifically for diesel engines: "DO NOT USE SAE 10W-40 GRADE OIL, OR ANY OTHER GRADE NOT RECOMMENDED".

If damage to an Oldsmobile diesel engine is caused by the use of SAE 10W-40 engine oil the cost of the engine repair will not be covered by the warranty.

#### API Engine Oil Service Symbol

A new API service symbol is being used in Oldsmobile owner's manuals and on oil cans. Urge your customers to look for it in their manuals and on the containers of the oil they select for use in their cars. See the illustration for examples of the symbol.

The symbol has an upper segment, center area, and lower segment. An explanation of the information in each of these locations is as follows:

Upper Segment: Quality Level ----------------------------

API (American Petroleum Institute) Service Categories

Gasoline Engines Diesel Engines ---------------- --------------

SF/CC SF/CD (preferred) SF/CD SF/CC SF

Center Area: OIL THICKNESS (Grade) ---------------------------------- SAE (Society of Automotive Engineers) viscosity Classification

Gasoline Engines Diesel Engines ---------------- ---------------

SAE 5W-30 (preferred for SAE 30 (preferred above engines of 2.8 liters of less). freezing).

SAE 10W-30 (preferred for SAE 10W-30 and SAE 15W-40 all other engines). (acceptable for all engines; use only for cold-weather operation; helps starting).

SAE 15W-40, SAE 20W-20 and SAE 30 (acceptable for all engines)

Lower Segment: FUEL ECONOMY RATING -------------

'ENERGY CONSERVING'

Oils with these words provide more miles per gallon of fuel.

The Goodwrench line of engine oils recently introduced by GM meets these standards and provides proper lubrication protection for passenger cars and light duty trucks.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.